William Li - Softproofing DevCon 08 Talk

The talk is primarily a walkthrough of the demo with a little bit of preamble, given the timeslot.  The theory surrounding this will also be presented by Dr. Chris Edge at CIC.
 

The demo setup will consist of 2 monitors flanking a small tabletop light booth.  One monitor will have been calibrated so that a spectroradiometer will read the same CIELab as the hard copy, the other will have been calibrated using a different method with different colorimetry.  The visible result is that some of the colors, especially in the blues, will be visibly different for the conventional CIELab based on 1931 tristimulus functions.  This demo was previously shown privately to the IDEAlliance Print Properties committee which was investigating soft proofing standards, and led to the tolerances and procedures which are currently in place for SWOP soft proofing certification owing to the acknowledged limitations of existing colorimetry.
 

The point of the demo is to reinforce a bit of caution on developers, that the act of matching monitor to proof is not necessarily as straightforward as they might think.
